|  |  |
| --- | --- |
| **To,** **Prof. Juerg M. Matter** Project Director, ODP | ***Doc. No.:*** *AZD/ODP/BT-1B/DPR-89****Dated:*** *23-03-2017* |
| **Client** | Oman DP | **Consultant** | AZD Engineering Consultancy |
| **Contractor** | Lalbuksh Voltas Engineering | **Sub-contractor** | Geo-Solutions Engineering |
| **Subject**  | Daily Progress Report |  |
| **Project** | **Phase-1: OmanDP -** Scientific Drilling Programme for Oman Drilling Project in Ash Sharqiyah North Governorate and Ad Dakhiliyah Governorate |

**DAILY PROGRESS REPORT**

**(Dated: 23rd of March 2017)**

|  |
| --- |
| **Rig-1 (Dynatech)** |
| ***LOCATION AND TARGET:*** |
| **Drill Hole ID** | **BT-1B**  | **Location** | **Wadi Mansah** |
| **Coordinates** | UTM 620988E 2584403N | **Elevation** | **-**  |
| **Azimuth** | N30°  | **Inclination** | Inclined 75° |
| **Drilling** | HQ Size | **Method** | Wire line-Diamond Core Drilling |
| **Target Depth**  | 400 mtrs | **Geol. Target** | Altered Peridotites-Basal Thrust |
| ***DRILLING:*** |
| **Drilling Status**  | Drill head constructed, site levelled and cleaned. All the completed core boxes moved to Muscat for storage. Drilling equipments and rig moved from the site; Site office, Generator, Camp etc., all transported to Muscat. Demobilization completed. |
| **Penetration Rate**  |  |
| **Bit Rotation**  |  |
| **Fluid Circulation**  |  |
| **Total Drill Run**  |  |
| **Today’s Drilling**  |  |
| **Cumulative Total**  | **300m (EOH)** *(1.9m for BT-1A)* |
| ***CORE CURATION:*** |
|  |
| ***PERSONNEL ONSITE:*** |
| **ODP :** Jude Coggon, David Zeko, Romain Lafay, Americus Perez, Juan Carlos**AZD :** Nehal Hasan Warsi**LBV :** Gopi Krishnan**GSE :** Sheikh Olliullah (D); Abdul Khaliq, Mohd. Jameel, Mohd. Sadiq etc**Others:** |
| ***REMARKS:***  |
| **\*Peter Kelemen leaves site.** |

Best Regards,

**Nehal H Warsi**

*Site Geologist, AZD Engineering Consultancy*

**GSM: +968 98037217; 79113454**

**Email: nhwarsi@gmail.com**