|  |  |
| --- | --- |
| **To,** **Prof. Juerg M. Matter** Project Director, ODP | ***Doc. No.:*** *AZD/ODP/GT-3A/DPR-70****Dated:*** *04-03-2017* |
| **Client** | Oman DP | **Consultant** | AZD Engineering Consultancy |
| **Contractor** | Lalbuksh Voltas Engineering | **Sub-contractor** | Geo-Solutions Engineering |
| **Subject**  | Daily Progress Report |  |
| **Project** | **Phase-1: OmanDP -** Scientific Drilling Programme for Oman Drilling Project in Ash Sharqiyah North Governorate and Ad Dakhiliyah Governorate |

**DAILY PROGRESS REPORT**

**(Dated: 4th of March 2017)**

|  |
| --- |
| **Rig-1 (Dynatech)** |
| ***LOCATION AND TARGET:*** |
| **Drill Hole ID** | **GT-3A**  | **Location** | **Wadi Abdah** |
| **Coordinates** | UTM: 624193.0E 2556476.0N | **Elevation** | **-** |
| **Azimuth** | **-** | **Inclination** | 90º/ Vertical |
| **Drilling** | HQ/NQ Size | **Method** | Wire line-Diamond Core Drilling |
| **Target Depth**  | 400 mtrs | **Geol. Target** | Sheeted Dyke-Gabbro Transition |
| ***DRILLING:*** |
| **Drilling Status**  | NC casing pulled out of hole. Well head constructed and Site rehabilitated. Rig and drilling accessories moved from GT-3 site to BT-1 site. Site camp setup at BT-1 site. |
| **Penetration Rate**  | - |
| **Bit Rotation**  | - |
| **Fluid Circulation**  | - |
| **Total Drill Run**  | - |
| **Today’s Drilling**  | **-** |
| **Cumulative Total**  | **400.00m**  *(HQ=257.3m; NQ=142.70m) EOH* |
| ***CORE CURATION:*** |
| **Brief Lithology: -**  |
| ***PERSONNEL ONSITE:*** |
| **ODP :** Peter Kelemen,Jude Coggon, David Zeko, Danial Nothaft, Romian Lafay, Eric**AZD :** Nehal Hasan Warsi**LBV :** Gopi Krishnan**GSE :** Sheikh Olliullah (D); Abdul Khaliq, Mohd. Jameel, Mohd. Alauddin and water tanker driver.**Others:** |
| ***REMARKS:***  |
| **\*Core boxes loaded onto the truck and moved to Muscat.** |

Best Regards,

**Nehal H Warsi**

*Site Geologist, AZD Engineering Consultancy*

**GSM: +968 98037217; 79113454**

**Email: nhwarsi@gmail.com**